<!doctype html public "-//w3c//dtd html 4.0 transitional//en">
<html>
<head>
   <meta http-equiv="Content-Type" content="text/html; charset=windows-1252">
   <meta http-equiv="Content-Language" content="en-gb">
   <meta name="robots" content="index,follow">
   <meta name="content" content="Image, Disk, Drive, Drive Image, Disk Image, Recover, Backup, Windows,DOS,FreeDOS,UDMA">
   <meta name="description" content="Drive SnapShot - how to make the bootable recovery disk">
   <meta name="keywords" content="Image, Disk, Drive, Drive Image, Disk Image, Recover, Backup, Windows,DOS,FreeDOS,UDMA">
   
   <title>Create a Dos boot disk</title>
<link rel="stylesheet" type="text/css" href="../css/snapshot.css">
   <base target="_parent">
</head>
<body>
<h2 align="center">Creation of a DOS BOOT floppy</h2>
<h3>If you have already a DOS Boot disk</h3>
<p>Fine. Just use it - Snapshot will run on any DOS. Just copy SNAPSHOT.EXE to
the disk and use it.</p>
<h3>If you are using&nbsp; Windows XP</h3>
<p>You can create a DOS Bootdisk by formatting a floppy with the Option 'MS-DOS
Bootdisk creation'.<br>
Windows XP will create a floppy, containing a (very limited) subset of Windows
ME.</p>
<h3>If you have SNAPSHOT installed</h3>
<p>
Snapshot SETUP has created a shortcut in the start menu
</p>
<p>
&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp; Programs-&gt;Snapshot Disk Imaging-&gt;Create
Disaster Recovery Disk.
</p>
<p>
Click this to create a bootable FreeDOS disk, including&nbsp; PnP network access
to your Windows server (see below).
</p>
<p>
If you bought the full version, you got a CDROM, which is bootable as well. The
booted CD is equivalent to the diskette above.
</p>
<p>Properties:<br>
&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;<br>
Always supported are FAT16, FAT32 und ATAPI CD-ROMs (the
<b>CDROM-Laufwerk </b>is as <b>W:</b>  installed)<span style="background-color: #C0C0C0">.</span>
</p>
<p>Due to limited available memory, you have to select on start, if you
additionally want to access local NTFS drives (for the image file location), or
want to find the image files on the Windows Network.
</p>
<h3> International Keyboard support</h3>
<p>When creating the recovery boot disk, Snapshot tries to detect the current
keyboard layout (of Windows). It then creates a file LANGUAGE.BAT on the
bootdisk, that is executed during boot and holds the statement</p>
<p>&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp; KEYB XX</p>
<p>where XX is the layout identifier to be loaded.&nbsp;<br>
Currently detected are English (US), United Kingdom (UK), German (GR), Swiss
German (SG), French (FR), Swiss French (SF), Portuguese (PO), Brazil (BR),
Russia (RU), Bulgaria (BG), Belgian (BE), Dutch (NL), Finnish (SU), Swedish (SV),
Italy (IT), Hebrew (HE), Norwegian (NO).<br>
You can get a list of all
supported layouts with&nbsp;</p>
<p>&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp; A:&gt;KEYB /L</p>
<h3>Bootdisk with PnP support for the Windows&nbsp; Network/Samba</h3>
<p>This Bootdisk is derived from <b>Bart Lagerweij's&nbsp;</b>  <a href="http://www.nu2.nu/bootdisk/network"><b>Bart's
Network Boot Disk</b></a>.&nbsp;<br>
We changed it to be based on FreeDOS to avoid license issues.</p>
<p>This disk supports</p>
<ul>
  <li><b>automatic detection</b> of your network adapter&nbsp;</li>
  <li>to use DHCP or direct selection of your IP Address</li>
  <li>TCP/IP or NetBEUI</li>
  <li>Save of Profiles to be available on next boot (only on diskette)</li>
</ul>
<p>After starting the disk, you have to enter something like&nbsp;</p>
<blockquote>
<p>A:&gt; NET USE&nbsp;&nbsp; Z:&nbsp;&nbsp; \\Servername\\Share</p>
</blockquote>
<p>and restore the image files from Z:</p>
<p>&nbsp;</p>
<blockquote>
  <p>Currently supported network adapters:</p>
</blockquote>
  <table class="nu2table" cellSpacing="1" cellPadding="2" border="1" width="740">
    <tbody>
      <tr>
        <th class="nu2th" width="170">File</th>
        <th class="nu2th" width="460">Description</th>
        <th class="nu2th" width="108">Updated</th>
      </tr>
      <tr>
        <td class="nu2td2" rowSpan="2" width="170"><a href="../nu2files/b57.uha">b57.uha</a>(19K)<br>
          <a href="../nu2files/b57.cab">b57.cab</a></td>
        <td class="nu2td2" width="460">Broadcom NetXtreme Gigabit Ethernet NDIS2
          Driver v8.23 (20 jul 05)</td>
        <td class="nu2td2" width="108">Aug 11, 2005</td>
      </tr>
      <tr>
        <td class="nu2td" colSpan="2" width="587"><b>Works also for HP/Compaq NC67xx/NC77xx Gigabit (Broadcom Based) adapters!</b></td>
      </tr>
      <tr>
        <td class="nu2td2" rowSpan="2" width="170">&nbsp;<a href="../nu2files/dc21x4.uha">dc21x4.uha</a>(19KB)<br>
          <a href="../nu2files/dc21x4.cab">cab</a></td>
        <td class="nu2td2" width="460">Digital 2104x/2114x 10/100 mbps Ethernet Controller
          v3.00</td>
        <td class="nu2td2" width="108">Mar 26, 2002</td>
      </tr>
      <tr>
        <td class="nu2td" colSpan="2" width="587">OEM: Linksys v1? Used in VirtualPC.</td>
      </tr>
      <tr>
        <td class="nu2td2" rowSpan="2" width="170"><a href="../nu2files/e100b.uha">e100b.uha</a>(12KB)<br>
          <a href="../nu2files/e100b.cab">e100b.cab</a></td>
        <td class="nu2td2" width="460">Intel(R) PRO PCI Driver v4.56 032404</td>
        <td class="nu2td2" width="108">Nov 11, 2005</td>
      </tr>
      <tr>
        <td class="nu2td" colSpan="2" width="587">v1.6 Updated by Todd Geib, added
          dev=1209,v1.7 Updated by BG,updated by Tom</td>
      </tr>
      <tr>
        <td class="nu2td2" rowSpan="2" width="170"><a href="../nu2files/E1000.uha">E1000.uha</a>(12KB)<br>
          <a href="../nu2files/E1000.cab">E1000.cab</a></td>
        <td class="nu2td2" width="460">Intel 8254X Based Adapter (pro/1000
          gigabit) v3.62 070204</td>
        <td class="nu2td2" width="108">Nov 11, 2005</td>
      </tr>
      <tr>
        <td class="nu2td" colSpan="2" width="587">Created by Todd Geib. Update by Dan
          Chappelear , BG,Tom.</td>
      </tr>
      <tr>
        <td class="nu2td2" width="170"><a href="../nu2files/el59x.uha">el59x.uha</a>(13KB)<br>
          <a href="../nu2files/el59x.cab">el59x.cab</a></td>
        <td class="nu2td2" width="460">3Com DOS NDIS driver for 3C59X Family Adapters v1.2f</td>
        <td class="nu2td2" width="108">Mar 26, 2002</td>
      </tr>
      <tr>
        <td class="nu2td2" rowSpan="2" width="170"><a href="../nu2files/el90x.uha">el90x.uha</a>(13KB)<br>
          <a href="../nu2files/el99x.cab">el99x.cab</a><br>
        </td>
        <td class="nu2td2" width="460">3Com Etherlink PCI DOS NDIS driver v5.2.2</td>
        <td class="nu2td2" width="108">Aug 15, 2002</td>
      </tr>
      <tr>
        <td class="nu2td" colSpan="2" width="587">Downgraded by Bob Whitworth (Nasa) with
          good reason: v5.2.5 for 3Com 90x cards doesn't work properly with old
          905-TX card (9050) with the original Parallel Tasking chip (not v2
          used in 905b or c). If you try to install Win2000 over the network, it
          will hang at random (usually about 40-60% thru). The 5.2.4 driver has
          the same bug. 3Com couldn't figure it out. The older v5.2.2 driver
          works with all 905s (905, 905b &amp; 905c).</td>
      </tr>
      <tr>
        <td class="nu2td2" rowSpan="2" width="170"><a href="../nu2files/elnk3.uha">elnk3.uha</a>&nbsp;(11KB)<br>
          <a href="../nu2files/elnk3.cab">elnk3.cab</a></td>
        <td class="nu2td2" width="460">3Com DOS EtherLink 10 ISA (3C509b) Network Driver
          v3.1</td>
        <td class="nu2td2" width="108">Sep 11, 2002</td>
      </tr>
      <tr>
        <td class="nu2td" colSpan="2" width="587">Updated by Dick Nagtegaal. Fixed divide
          overflow on fast Pentium machines. <a title="http://support.3com.com/infodeli/tools/nic/3c509b.htm" href="http://support.3com.com/infodeli/tools/nic/3c509b.htm" target="_blank">More
          info!</a></td>
      </tr>
      <tr>
        <td class="nu2td2" rowSpan="2" width="170"><a href="../nu2files/elpc3.uha">elpc3.uha</a>(14KB)<br>
          <a href="../nu2files/elpc3.cab">elpc3.cab</a></td>
        <td class="nu2td2" width="460">3Com Megahertz Ethernet PC Card 589E DOS Network
          Driver v1.9.005</td>
        <td class="nu2td2" width="108">Feb 3, 2003</td>
      </tr>
      <tr>
        <td class="nu2td" colSpan="2" width="587">Updated by Robert Mader. Should fix divide
          by zero errors. <a title="http://help.nec-computers.com/uk/itemnr/NECFIUP03730100.asp" href="http://help.nec-computers.com/uk/itemnr/NECFIUP03730100.asp" target="_blank">More
          info!</a></td>
      </tr>
      <tr>
        <td class="nu2td2" width="170"><a href="../nu2files/elpc575.uha">elpc575.uha</a>(14KB)<br>
          <a href="../nu2files/elpc575.cab">elpc575.cab</a></td>
        <td class="nu2td2" width="460">3Com Megahertz 10/100 LAN CardBus PC Card DOS NDIS
          driver v3.4b</td>
        <td class="nu2td2" width="108">Mar 26, 2002</td>
      </tr>
      <tr>
        <td class="nu2td2" width="170"><a href="../nu2files/getnd2.uha">getnd2.uha</a>&nbsp;(9KB)<br>
          <a href="../nu2files/getnd2.cab">getnd2.cab</a></td>
        <td class="nu2td2" width="460">VIA Networking Velocity Family Gigabit Ethernet Adapter v1.05 (09/08/03)</td>
        <td class="nu2td2" width="108">Dec 18, 2004</td>
      </tr>
      <tr>
        <td class="nu2td2" width="170"><a href="../nu2files/ne2000.uha">ne2000.uha</a>&nbsp;(9KB)<br>
          <a href="../nu2files/ne2000.cab">ne2000.cab</a></td>
        <td class="nu2td2" width="460">Microsoft NE2000 NDIS Driver</td>
        <td class="nu2td2" width="108">Jul 11, 2002</td>
      </tr>
      <tr>
        <td class="nu2td2" width="170"><a href="../nu2files/nc100.uha">nc100.uha</a>&nbsp;(13KB)<br>
          <a href="../nu2files/nc100.cab">nc100.cab</a></td>
        <td class="nu2td2" width="460">Compaq Fast Ethernet and Gigabit NDIS 2
          NIC Drivers 7.0a (25Jan02)</td>
        <td class="nu2td2" width="108">Mar 26, 2002</td>
      </tr>
      <tr>
        <td class="nu2td" width="170">&nbsp;</td>
        <td class="nu2td" width="437">Created by Dilan Patel</td>
      </tr>
      <tr>
        <td class="nu2td2" rowSpan="2" width="170"><a href="../nu2files/n1000.uha">n1000.uha</a>&nbsp;(12KB)<br>
          <a href="../nu2files/n1000.cab">n1000.cab</a></td>
        <td class="nu2td2" width="460">Compaq Gigabit 6134/6136 (Intel Based)</td>
        <td class="nu2td2" width="108">Mar 26, 2002</td>
      </tr>
      <tr>
        <td class="nu2td" colSpan="2" width="587">Created by Dimitri Janczak.
          Does not support EMM386!</td>
      </tr>
      <tr>
        <td class="nu2td2" width="170"><a href="../nu2files/pcntnd.uha">pcntnd.uha</a>&nbsp;(13KB)<br>
          <a href="../nu2files/pcntnd.cab">pcntnd.cab</a></td>
        <td class="nu2td2" width="460">AMD PCNet Family Ethernet Adapter NDIS v2.0.1 MAC
          Driver v3.12</td>
        <td class="nu2td2" width="108">Mar 26, 2002</td>
      </tr>
      <tr>
        <td class="nu2td2" width="170"><a href="../nu2files/rtsnd.uha">rtsnd.uha</a>&nbsp;(21KB)<br>
          <a href="../nu2files/rtsnd.cab">rtsnd.cab</a></td>
        <td class="nu2td2" width="460">Realtek RTL8139/810X Family PCI Fast Ethernet v3.23
          07/28/99</td>
        <td class="nu2td2" width="108">Mar 26, 2002</td>
      </tr>
      <tr>
        <td class="nu2td2" width="170"><a href="../nu2files/RTGBND.uha">RTGBND.uha</a>&nbsp;(8KB)<br>
          <a href="../nu2files/RTGBND.cab">RTGBND.cab</a></td>
        <td class="nu2td2" width="460">RTL8169/8110 Family Gigabit Ethernet Adapter v1.01 (07/16/03)(Tom)</td>
        <td class="nu2td2" width="108">Dec 18,2004</td>
      </tr>
      <tr>
        <td class="nu2td2" width="170"><a href="../nu2files/sis900.uha">sis900.uha</a>&nbsp;(14KB)<br>
          <a href="../nu2files/sis900.cab">sis900.cab</a></td>
        <td class="nu2td2" width="460">SiS 900/7016 SIS900 10/100 PCI DOS Driver v1.13</td>
        <td class="nu2td2" width="108">Mar 26, 2002</td>
      </tr>
      <tr>
        <td class="nu2td2" width="170"><a href="../nu2files/smc9432.uha">smc9432.uha</a>&nbsp;(13KB)<br>
          <a href="../nu2files/smc9432.cab">smc9432.cab</a></td>
        <td class="nu2td2" width="460">SMC EtherPower II 10/100 (9432TX) v1.02c (970605)</td>
        <td class="nu2td2" width="108">Mar 26, 2002</td>
      </tr>
      <tr>
        <td class="nu2td2" width="170"><a href="../nu2files/yuknd.uha">yuknd.uha</a>&nbsp;(26KB)<br>
          <a href="../nu2files/yuknd.cab">yuknd.cab</a></td>
        <td class="nu2td2" width="460">Yukon Marvel / SysKonnect SK-9872 / 3Com
          3C2000T&nbsp;<br>
          Gigabit NDIS2 Driver v7.05 (06/15/04)</td>
        <td class="nu2td2" width="108">Nov 11, 2005</td>
      </tr>
      <tr>
        <td class="nu2td2" width="170">D-LINK&nbsp;(0KB)</td>
        <td class="nu2td2" width="460">D-Link DGE-530T Gigabit : doesn't support
          DOS - hands off !! (tom)</td>
        <td class="nu2td2" width="108">Dec 18, 2004</td>
      </tr>
    </tbody>
  </table>
<p>If you have a different Network adapter, go to <a href="#morenics"><b>More
Network Drivers</b></a>.<br>
You will find ~100 supported drivers, which unfortunately don't fit all on a
floppy disk. Just copy the required driver XXXCARD.CAB into A:\LIB\NDIS, and
reboot.</p>
<blockquote>
  <p>We would like to hear from you, which drivers are missing; so we can place
  the most required drivers immediately into the delivered package.<a href="mailto:support@drivesnapshot.de?subject=SNAPSHOT-missing%20Network-driver&body=Hallo%0d%0a,we use the Network Card:">
<br>
  short note to support@drivesnapshot.de</a>  will do. thanks.</p>
</blockquote>
<h3><a name="NTFSDOS"></a>NTFS Support for DOS</h3>
<p>If your image files are located on a NTFS volume, DOS isn't able to access
them by itself.</p>
<p><a href="http://www.sysinternals.com" target="_blank"><b>Sysinternals</b></a> 
 offers (besides a lot of different useful utilities) a&nbsp; <b><a href="http://www.sysinternals.com/ntw2k/freeware/NTFSDOS.shtml">NTFSDOS</a></b> 
 driver for DOS; the read-only variant is free.</p>
<p>Please download NTFSDOS.EXE&nbsp; and copy it to&nbsp; A:\UTILS.&nbsp;</p>
<p>Due to License issues, we are not allowed to add it to our delivery package
(coming soon).<br>
</p>
<h3>UDMA Support for DOS</h3>
<p>Most motherboard don't support the fast UDMA mode for IDE drives in their
BIOS; therefore Disk transfer speed in DOS is limited to ~8MB/sec, which results
in a max. possible restore rate of 5MB/sec.&nbsp;</p>
<p>Modern hard disks could have a transfer speed of 50 MB/sec and more, if
accessed with UDMA.</p>
<p>UDMA will test it's functionality, and will not load, if it doesn't find compatible
hardware. Unfortunately, the test causes some (very few) main boards to hang, so
we can't load it automatically.</p>
<p>UDMA was developed by&nbsp; Jack Ellis - thanks for that :))<br>
</p>
<h3>More Network Drivers</h3>
<p>Unfortunately not all existing network card drivers fit on a single floppy;
here are ~100 more supported.<br>
Just&nbsp;<br>
&nbsp;&nbsp;&nbsp; download<br>
&nbsp;&nbsp;&nbsp; copy to a:\lib\ndis<br>
&nbsp;&nbsp;&nbsp; reboot</p>
<br>
<table class="nu2table" cellSpacing="1" cellPadding="2" border="1" width="740">
  <tbody>
    <tr>
      <th class="nu2th">File</th>
      <th class="nu2th">Description</th>
      <th class="nu2th">Updated</th>
    </tr>
    <tr>
        <td class="nu2td2" rowSpan="2" width="170"><a href="../nu2files/E1000.uha">E1000.uha</a>
          <a href="../nu2files/E1000.cab">cab</a>(12KB)</td>
        <td class="nu2td2" width="460">Intel 8254X Based Adapter (pro/1000
          gigabit) v3.62 070204</td>
        <td class="nu2td2" width="108">Nov 11, 2005</td>
    </tr>
    <tr>
        <td class="nu2td" colSpan="2" width="587">Created by Todd Geib. Update by Dan
          Chappelear , BG,Tom.</td>
    </tr>
    <tr>
        <td class="nu2td2" rowSpan="2" width="170"><a href="../nu2files/e100b.uha">e100b.uha</a>
          <a href="../nu2files/e100b.cab">cab</a>(12KB)</td>
        <td class="nu2td2" width="460">Intel(R) PRO PCI Driver v4.56 032404</td>
        <td class="nu2td2" width="108">Nov 11, 2005</td>
    </tr>
    <tr>
        <td class="nu2td" colSpan="2" width="587">v1.6 Updated by Todd Geib, added
          dev=1209,v1.7 Updated by BG,updated by Tom</td>
    </tr>
    <tr>
        <td class="nu2td2" rowSpan="2" width="170"><a href="../nu2files/b57.uha">b57.uha</a>
          <a href="../nu2files/b57.cab">cab</a>(19K)</td>
        <td class="nu2td2" width="460">Broadcom NetXtreme Gigabit Ethernet NDIS2
          Driver v8.23 (20 jul 05)</td>
        <td class="nu2td2" width="108">Aug 11, 2005</td>
    </tr>
    <tr>
        <td class="nu2td" colSpan="2" width="587"><b>Works also for HP/Compaq NC67xx/NC77xx Gigabit (Broadcom Based) adapters!</b></td>
    </tr>
    <tr>
        <td class="nu2td2" width="170"><a href="../nu2files/yuknd.uha">yuknd.uha</a>&nbsp;<a href="../nu2files/yuknd.cab">cab</a>(26KB)<br>
      </td>
        <td class="nu2td2" width="460">Yukon Marvel / SysKonnect SK-9872 / 3Com
          3C2000T&nbsp;<br>
          Gigabit NDIS2 Driver v7.05 (06/15/04)</td>
        <td class="nu2td2" width="108">Nov 11, 2005</td>
    </tr>
    <tr>
      <td class="nu2td2"><a href="../nu2files/dp83815.uha">dp83815.uha</a>&nbsp;<a href="../nu2files/dp83815.cab">cab</a>(15KB)</td>
      <td class="nu2td2">DP83815 10/100 MacPhyter PCI Adapters DOS v1.16</td>
      <td class="nu2td2">Nov 12, 2003</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Mirando K. OEM: Netgear
        FA311/FA312<br>
        v1.1: Updated by Peter Verstraten.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/b44.uha">b44.uha</a>&nbsp;<a href="../nu2files/b44.cab">b44.cab</a>(15KB)</td>
      <td class="nu2td2">Broadcom 440x 10/100 Ethernet NDIS2 Driver v2.44
        (030506)</td>
      <td class="nu2td2">Jul 8, 2003</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by K. Stulen from HP<br>
      </td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/elpc3.uha">elpc3.uha</a>&nbsp;<a href="../nu2files/elpc3.cab">elpc3.cab</a>(14KB)</td>
      <td class="nu2td2">3Com Megahertz Ethernet PC Card 589E DOS Network Driver
        v1.9.005</td>
      <td class="nu2td2">Feb 3, 2003</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Updated by Robert Mader. Should fix divide
        by zero errors. <a title="http://help.nec-computers.com/uk/itemnr/NECFIUP03730100.asp" href="http://help.nec-computers.com/uk/itemnr/NECFIUP03730100.asp" target="_blank">More
        info!</a></td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/exp16.uha">exp16.uha</a>&nbsp;<a href="../nu2files/exp16.cab">exp16.cab</a>
        (6KB)</td>
      <td class="nu2td2">Intel EtherExpress 16 ISA Driver v2.36</td>
      <td class="nu2td2">Jun 13, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Oliver Hookins.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/m16andis.uha">m16andis.uha</a>&nbsp;<a href="../nu2files/m16andis.cab">m16andis.cab</a>(17KB)</td>
      <td class="nu2td2">Intel EtherExpress PRO/100 PC Card Mobile Adapter16
        Driver v1.61 (970702)</td>
      <td class="nu2td2">Jun 12, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Jay Davis.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/el99x.uha">el99x.uha</a>&nbsp;<a href="../nu2files/el90x.uha">el90x.uha</a>(34KB)</td>
      <td class="nu2td2">3Com Etherlink 10/100 PCI Adapter with 3XP (3C990)</td>
      <td class="nu2td2">Jun 3, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Al Gilhousen.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/el90x.uha">el90x.uha</a>&nbsp;<a href="../nu2files/el90x.uha">el90x.uha</a>(13KB)</td>
      <td class="nu2td2">3Com Etherlink PCI DOS NDIS driver v5.2.2</td>
      <td class="nu2td2">Aug 15, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Downgraded by Bob Whitworth (Nasa) with good
        reason: v5.2.5 for 3Com 90x cards doesn't work properly with old 905-TX
        card (9050) with the original Parallel Tasking chip (not v2 used in 905b
        or c). If you try to install Win2000 over the network, it will hang at
        random (usually about 40-60% thru). The 5.2.4 driver has the same bug.
        3Com couldn't figure it out. The older v5.2.2 driver works with all 905s
        (905, 905b &amp; 905c).</td>
    </tr>
    <tr>
      <td class="nu2td2"><a href="../nu2files/el59x.uha">el59x.uha</a>&nbsp;<a href="../nu2files/el59x.cab">el59x.cab</a>(13KB)</td>
      <td class="nu2td2">3Com DOS NDIS driver for 3C59X Family Adapters v1.2f</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/elnk3.uha">elnk3.uha</a>&nbsp;<a href="../nu2files/elnk3.cab">elnk3.cab</a>(11KB)</td>
      <td class="nu2td2">3Com DOS EtherLink 10 ISA (3C509b) Network Driver v3.1</td>
      <td class="nu2td2">Sep 11, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Updated by Dick Nagtegaal. Fixed divide
        overflow on fast Pentium machines. <a title="http://support.3com.com/infodeli/tools/nic/3c509b.htm" href="http://support.3com.com/infodeli/tools/nic/3c509b.htm" target="_blank">More
        info!</a></td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/elpc3.uha">elpc3.uha</a>&nbsp;<a href="../nu2files/elpc3.cab">elpc3.cab</a>(17KB)</td>
      <td class="nu2td2">3Com EtherLink III LAN+Modem PC Card (3c562)</td>
      <td class="nu2td2">Aug 15, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Todd George.</td>
    </tr>
    <tr>
      <td class="nu2td2"><a href="../nu2files/elpc575.uha">elpc575.uha</a>&nbsp;<a href="../nu2files/elpc575.cab">elpc575.cab</a>(14KB)</td>
      <td class="nu2td2">3Com Megahertz 10/100 LAN CardBus PC Card DOS NDIS
        driver v3.4b</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/el556.uha">el556.uha</a>&nbsp;<a href="../nu2files/el556.cab">el556.cab</a>(12KB)</td>
      <td class="nu2td2">3Com EL556 driver 10/100 V.90 Mini-PCI Combo Card Jan
        22, 2001</td>
      <td class="nu2td2">Jun 6, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by John Ole Gronmo. Updated v1.1:
        added device 6056 to ndis.pci by Bob Gagnon.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a title="/download.php?sFile=elpc656.cab" href="http://www.nu2.nu/download.php?sFile=elpc656.cab">elpc656.cab</a>&nbsp;(13KB)</td>
      <td class="nu2td2">3Com 3C656 10/100 LAN+56K CardBus PC Card</td>
      <td class="nu2td2">Aug 15, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Todd George.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/fem556.uha">fem556.uha</a>&nbsp;<a href="../nu2files/fem556.cab">fem556.cab</a>(18KB)</td>
      <td class="nu2td2">3Com Megahertz Ethernet 3CCFEM556B</td>
      <td class="nu2td2">May 22, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Geoffrey Gardner. For the 3Com
        Megahertz 10/100 Lan+56K Modem PC Card Model 3CCFEM556 B Ver.1.1.1</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/el3c574.uha">el3c574.uha</a>&nbsp;<a href="../nu2files/el3c574.cab">el3c574.cab</a>(15KB)</td>
      <td class="nu2td2">3Com-Megahertz 574 LAN PC Card Dos NDIS Driver v1.2.005</td>
      <td class="nu2td2">May 31, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Patrick Fortin-Ducharme. Updated
        by Dustin Krysak.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/el515.uha">el515.uha</a>&nbsp;<a href="../nu2files/el515.cab">el515.cab</a>(13KB)</td>
      <td class="nu2td2">3Com 3C515-TX Fast Etherlink ISA PnP</td>
      <td class="nu2td2">Apr 23, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Lou Vaccari</td>
    </tr>
    <tr>
      <td class="nu2td2"><a href="../nu2files/netflx3.uha">netflx3.uha</a>&nbsp;<a href="../nu2files/netflx3.cab">netflx3.cab</a>(31KB)</td>
      <td class="nu2td2">Compaq NetFlex-3 DOS NDIS 2.02 driver</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/n100.uha">n100.uha</a>&nbsp;<a href="../nu2files/n100.cab">n100.cab</a>(13KB)</td>
      <td class="nu2td2">Compaq Fast Ethernet and Gigabit NDIS 2 NIC Drivers
        7.0a (25Jan02)</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Dilan Patel</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/n1000.uha">n1000.uha</a>&nbsp;<a href="../nu2files/n1000.cab">n1000.cab</a>(12KB)</td>
      <td class="nu2td2">Compaq Gigabit 6134/6136 (Intel Based)</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Dimitri Janczak. Does not support
        EMM386!</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/pcntnd.uha">pcntnd.uha</a>&nbsp;<a href="../nu2files/pcntnd.cab">pcntnd.cab</a>(13KB)</td>
      <td class="nu2td2">AMD PCNet Family Ethernet Adapter NDIS v2.0.1 MAC
        Driver v3.12</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Used in VMWare.</td>
    </tr>
    <tr>
      <td class="nu2td2"><a href="../nu2files/smc9432.uha">smc9432.uha</a>&nbsp;<a href="../nu2files/smc9432.cab">smc9432.cab</a>(13KB)</td>
      <td class="nu2td2">SMC EtherPower II 10/100 (9432TX) v1.02c (970605)</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/smc8000.uha">smc8000.uha</a>&nbsp;<a href="../nu2files/smc8000.cab">smc8000.cab</a>(17KB)</td>
      <td class="nu2td2">SMC EtherCard PLUS NDIS Driver v4.06a (SMC8xxx)</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Allard Sijm. Also supports the
        old SMC/WD8003 and 8013 ISA cards the SMC EtherCard Elite 16 Ultra (8216
        series) and EtherEZ (8416 series).</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/smc1660.uha">smc1660.uha</a>&nbsp;<a href="../nu2files/smc1660.cab">smc1660.cab</a>(9KB)</td>
      <td class="nu2td2">SMC EZ Card 10 ISA (SMC 1660 Series)</td>
      <td class="nu2td2">Jul 5, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Robert Cooper</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/smc1255.uha">smc1255.uha</a>&nbsp;<a href="../nu2files/smc1255.cab">smc1255.cab</a>(8KB)</td>
      <td class="nu2td2">SMC EZ Card 10/100 PCI (SMC1255 Series)</td>
      <td class="nu2td2">Jul 5, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Robert Cooper</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/smc1208.uha">smc1208.uha</a>&nbsp;<a href="../nu2files/smc1208.cab">smc1208.cab</a>(6KB)</td>
      <td class="nu2td2">SMC EZ Card 10 PCI (SMC1208 Series)</td>
      <td class="nu2td2">Jul 5, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Robert Cooper</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/smc1211.uha">smc1211.uha</a>&nbsp;<a href="../nu2files/smc1211.cab">smc1211.cab</a>(21KB)</td>
      <td class="nu2td2">SMC EZ Card 10/100 PCI (SMC1211 Series)</td>
      <td class="nu2td2">Apr 10, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Shane Brooks</td>
    </tr>
    <tr>
      <td class="nu2td2"><a href="../nu2files/sis900.uha">sis900.uha</a>&nbsp;<a href="../nu2files/sis900.cab">sis900.cab</a>(14KB)</td>
      <td class="nu2td2">SiS 900/7016 SIS900 10/100 PCI DOS Driver v1.13</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/cbendis.uha">cbendis.uha</a>&nbsp;<a href="../nu2files/cbendis.cab">cbendis.cab</a>(24KB)</td>
      <td class="nu2td2">Xircom CardBus Ethernet 10/100 Adapter</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Michel Harding</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/ce3ndis.uha">ce3ndis.uha</a>&nbsp;<a href="../nu2files/ce3ndis.cab">ce3ndis.cab</a>(24KB)</td>
      <td class="nu2td2">Xircom Ethernet 10/100 (CE3)</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Tim Vanlint</td>
    </tr>
    <tr>
      <td class="nu2td2"><a href="../nu2files/xcemndis.uha">xcemndis.uha</a>&nbsp;<a href="../nu2files/xcemndis.cab">xcemndis.cab</a>(24KB)</td>
      <td class="nu2td2">Xircom Ethernet 10/100+Modem 56 Adapter (XEM)</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/rem56g10.uha">rem56g10.uha</a>&nbsp;<a href="../nu2files/rem56g10.cab">rem56g10.cab</a>(24KB)</td>
      <td class="nu2td2">Xircom Realport Ethernet + Modem 56 (REM56G-10)</td>
      <td class="nu2td2">Apr 23, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Patrick Baeken</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/xircom.uha">xircom.uha</a>&nbsp;<a href="../nu2files/xircom.cab">xircom.cab</a>(22KB)</td>
      <td class="nu2td2">Xircom Pocket Ethernet Adapter III</td>
      <td class="nu2td2">Sep 4, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Hon Chau.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/mxnicf.uha">mxnicf.uha</a>&nbsp;<a href="../nu2files/mxnicf.cab">mxnicf.cab</a>(7KB)</td>
      <td class="nu2td2">Macronix MX987xx Family Fast Ethernet NDIS 2 MAC</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Howard F. Cooper</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/dm9pci.uha">dm9pci.uha</a>&nbsp;<a href="../nu2files/dm9pci.cab">dm9pci.cab</a>(9KB)</td>
      <td class="nu2td2">DAVICOM DM9PCI Series Ethernet Adapter v1.28</td>
      <td class="nu2td2">Jun 6, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Art Heimsoth. Updated v1.1:
        Driver file now v1.28 by Jack Spradling.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/accnd.uha">accnd.uha</a>&nbsp;<a href="../nu2files/accnd.cab">accnd.cab</a>(21KB)</td>
      <td class="nu2td2">Accton EN1207D-TX/EN2242A Series Fast-Ethernet PCI
        Adapter</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Mike Elliott</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/en5251.uha">en5251.uha</a>&nbsp;<a href="../nu2files/en5251.cab">en5251.cab</a>(8KB)</td>
      <td class="nu2td2">Accton EN5251 Based Fast Ethernet Adapter Driver v1.04</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Chris Porosky</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/lm560txc.uha">lm560txc.uha</a>&nbsp;<a href="../nu2files/lm560txc.cab">lm560txc.cab</a>(17KB)</td>
      <td class="nu2td2">Accton ComNet56k PCMCIA 10/100 Ethernet + Modem</td>
      <td class="nu2td2">Apr 5, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Tomasz Saniawa. The enabler uses
        IRQ 11 and port 300h.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/ethne.uha">ethne.uha</a>&nbsp;<a href="../nu2files/ethne.cab">ethne.cab</a>(9KB)</td>
      <td class="nu2td2">Accton EN166x MPX2 PnP Ethernet Adapter EtherCombo/Coax/Pair</td>
      <td class="nu2td2">Jul 5, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Severin TERRIER</td>
    </tr>
    <tr>
      <td class="nu2td2"><a href="../nu2files/l100.uha">l100.uha</a>&nbsp;<a href="../nu2files/l100.cab">l100.cab</a>(7KB)</td>
      <td class="nu2td2">Lite-on PNIC-10/100 (Fast) Ethernet Adapter v3.0</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/lne100d.uha">lne100d.uha</a>&nbsp;<a href="../nu2files/lne100d.cab">lne100d.cab</a>(13KB)</td>
      <td class="nu2td2">Linksys LNE100TX Fast Ethernet Adapter (Chip Name:
        Digital)</td>
      <td class="nu2td2">Jun 25, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">With IC Chip from Digital. Created by Jeff
        Bogari. <a title="http://linksys.com/download/driver.asp?dlid=2&amp;osid=2" href="http://linksys.com/download/driver.asp?dlid=2&amp;osid=2" target="_blank">More
        info!</a></td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/lne100l.uha">lne100l.uha</a>&nbsp;<a href="../nu2files/lne100l.cab">lne100l.cab</a>(7KB)</td>
      <td class="nu2td2">Linksys LNE100TX Fast Ethernet Adapter (Chip Name:
        Linksys)</td>
      <td class="nu2td2">Jun 25, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">With IC Chip from Linksys. Created by Jeff
        Bogari. <a title="http://linksys.com/download/driver.asp?dlid=2&amp;osid=2" href="http://linksys.com/download/driver.asp?dlid=2&amp;osid=2" target="_blank">More
        info!</a></td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/lne100p.uha">lne100p.uha</a>&nbsp;<a href="../nu2files/lne100p.cab">lne100p.cab</a>(7KB)</td>
      <td class="nu2td2">Linksys LNE100TX Fast Ethernet Adapter (Chip Name: PNIC)</td>
      <td class="nu2td2">Jun 25, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">With IC Chip from PNIC. Created by Jeff
        Bogari. <a title="http://linksys.com/download/driver.asp?dlid=2&amp;osid=2" href="http://linksys.com/download/driver.asp?dlid=2&amp;osid=2" target="_blank">More
        info!</a></td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/lne100v2.uha">lne100v2.uha</a>&nbsp;<a href="../nu2files/lne100v2.cab">lne100v2.cab</a>(9KB)</td>
      <td class="nu2td2">Linksys LNE100TX v2 Fast Ethernet Adapter (LNE100)</td>
      <td class="nu2td2">Jun 11, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">This is for the version 2.0 adapter! Created
        by Victor Grund, updated using info from Jeff Bogari. <a title="http://linksys.com/download/driver.asp?dlid=2&amp;osid=2" href="http://linksys.com/download/driver.asp?dlid=2&amp;osid=2" target="_blank">More
        info!</a></td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/lne100v4.uha">lne100v4.uha</a>&nbsp;<a href="../nu2files/lne100v4.cab">lne100v4.cab</a>(8KB)</td>
      <td class="nu2td2">Linksys LNE100TX v4 Fast Ethernet Adapter</td>
      <td class="nu2td2">Jun 11, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">This is for the version 4.x adapter! Created
        by Jeff Bogari. <a title="http://linksys.com/download/driver.asp?dlid=2&amp;osid=2" href="http://linksys.com/download/driver.asp?dlid=2&amp;osid=2" target="_blank">More
        info!</a></td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/lne100v5.uha">lne100v5.uha</a>&nbsp;<a href="../nu2files/lne100v5.cab">lne100v5.cab</a>(8KB)</td>
      <td class="nu2td2">Linksys LNE100TX v5 Fast Ethernet Adapter</td>
      <td class="nu2td2">Jun 25, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">This is for the version 5.x adapter! Created
        by Jeff Bogari. <a title="http://linksys.com/download/driver.asp?dlid=2&amp;osid=2" href="http://linksys.com/download/driver.asp?dlid=2&amp;osid=2" target="_blank">More
        info!</a></td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/n100.uha">n100.uha</a>&nbsp;<a href="../nu2files/n100.cab">n100.cab</a>(8KB)</td>
      <td class="nu2td2">Linksys NC100 (Network Everywhere Fast Eth. Adap. NC100
        v2)</td>
      <td class="nu2td2">May 21, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Paul McEwan and David Coulter.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/pc100.uha">pc100.uha</a>&nbsp;<a href="../nu2files/pc100.cab">pc100.cab</a>(14KB)</td>
      <td class="nu2td2">Linksys EtherFast 10/100 PC Card (PCMPC100) NDIS DOS
        Driver v2.20</td>
      <td class="nu2td2">Aug 15, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Federico Lucifredi. Enabler
        options are set to &quot;/IOP=320 /IRQ=11&quot;.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/ec2t.uha">ec2t.uha</a>&nbsp;<a href="../nu2files/ec2t.cab">ec2t.cab</a>(13KB)</td>
      <td class="nu2td2">Linksys Combo PCMCIA Adapter</td>
      <td class="nu2td2">May 21, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Craig Setera. The card services
        enabler is set with paramters IOP=300 and IRQ=11</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/le10nds.uha">le10nds.uha</a>&nbsp;<a href="../nu2files/le10nds.cab">le10nds.cab</a>(13KB)</td>
      <td class="nu2td2">EPC-0100 TB Level-One PC Card / PCMCIA 10Mbps</td>
      <td class="nu2td2">Apr 24, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by René Beer. Uses I/O port 0x300
        and IRQ 5. <a title="http://www.level-one.net" href="http://www.level-one.net" target="_blank">More
        info!</a></td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/pcntnd.uha">pcntnd.uha</a>&nbsp;<a href="../nu2files/pcntnd.cab">pcntnd.cab</a>(6KB)</td>
      <td class="nu2td2">Realtek 8019 driver v2.0</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Robert Moosreiner</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/pcind.uha">pcind.uha</a>&nbsp;<a href="../nu2files/pcind.cab">pcind.cab</a>(7KB)</td>
      <td class="nu2td2">Realtek RTL8029 Family PCI Fast Ethernet</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Dennis Descheneaux</td>
    </tr>
    <tr>
      <td class="nu2td2"><a href="../nu2files/rtsnd.uha">rtsnd.uha</a>&nbsp;<a href="../nu2files/rtsnd.cab">rtsnd.cab</a>(21KB)</td>
      <td class="nu2td2">Realtek RTL8139/810X Family PCI Fast Ethernet v3.23
        07/28/99</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/de22x.uha">de22x.uha</a>&nbsp;<a href="../nu2files/de22x.cab">de22x.cab</a>(12KB)</td>
      <td class="nu2td2">D-Link DE-220 Family Ethernet NDIS DOS Driver v5.01</td>
      <td class="nu2td2">Aug 30, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Aleksandr A. Kozlov. This is ISA
        PnP NIC, that I used in PnP mode, so I have no ideas about it will work
        when NIC is non-PnP mode.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/dlkrts.uha">dlkrts.uha</a>&nbsp;<a href="../nu2files/dlkrts.cab">dlkrts.cab</a>(21KB)</td>
      <td class="nu2td2">D-Link DFE-530TX+ 10/100 Fast/Eth v5.390</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Jose Raul Cruz R.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/dlh5x.uha">dlh5x.uha</a>&nbsp;<a href="../nu2files/dlh5x.cab">dlh5x.cab</a>(10KB)</td>
      <td class="nu2td2">D-Link DFE-550TX 10/100 Adapter NDIS2 v1.06</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Dennis Descheneaux</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/de620.uha">de620.uha</a>&nbsp;<a href="../nu2files/de620.cab">de620.cab</a>(10KB)</td>
      <td class="nu2td2">D-Link DE-620CT Ethernet Pocket LAN Adapter</td>
      <td class="nu2td2">Aug 30, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Crisco.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/de660.uha">de660.uha</a>&nbsp;<a href="../nu2files/de660.cab">de660.cab</a>(11KB)</td>
      <td class="nu2td2">D-Link DE-660 Ethernet PC Card Driver v2.10</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Jan Drost</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/dfe650.uha">dfe650.uha</a>&nbsp;<a href="../nu2files/dfe650.cab">dfe650.cab</a>(13KB)</td>
      <td class="nu2td2">D-Link DFE-650 Fast Ethernet PC Card Driver v1.02</td>
      <td class="nu2td2">Jun 13, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Jeremy Ferris</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/dfe660.uha">dfe660.uha</a>&nbsp;<a href="../nu2files/dfe660.cab">dfe660.cab</a>(19KB)</td>
      <td class="nu2td2">D-Link DFE-660(TX) PCMCIA Ethernet 10/100 v1.12</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Pedro Rodrigues</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/dfe670.uha">dfe670.uha</a>&nbsp;<a href="../nu2files/dfe670.cab">dfe670.cab</a>(16KB)</td>
      <td class="nu2td2">D-Link DFE-670TXD 10/100 PCMCIA card</td>
      <td class="nu2td2">Jul 5, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Bob Leonard</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/dlkpci.uha">dlkpci.uha</a>&nbsp;<a href="../nu2files/dlkpci.cab">dlkpci.cab</a>(18KB)</td>
      <td class="nu2td2">D-Link PCI DEC2104x/2114x 10/100 mbps Ethernet v2.61</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Pedro Rodrigues. Note: Same PCI
        vendor/device id's as dc21x4! But the dc21x4 driver doesn't work with
        the D-Link DFE500TX card</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/dc21x4.uha">dc21x4.uha</a>&nbsp;(<a href="../nu2files/dc21x4.cab">dc21x4.cab</a>19KB)</td>
      <td class="nu2td2">Digital 2104x/2114x 10/100 mbps Ethernet Controller
        v3.00</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">OEM: Linksys v1? Used in VirtualPC.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/fetnd.uha">fetnd.uha</a>&nbsp;<a href="../nu2files/fetnd.cab">fetnd.cab</a>(10KB)</td>
      <td class="nu2td2">VIA Rhine Family Fast Ethernet Adapter Driver v4.05</td>
      <td class="nu2td2">Aug 30, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">v1.1: Updated by Brett King.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/w940nd.uha">w940nd.uha</a>&nbsp;<a href="../nu2files/w940nd.cab">w940nd.cab</a>(6KB)</td>
      <td class="nu2td2">Winbond W89C940F 10 PCI DOS Driver v2.00</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Robert Moosreiner</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2">&nbsp;<a href="../nu2files/ne2000.uha">ne2000.uha</a>
        <a href="../nu2files/ne2000.cab">ne2000.cab</a>(9KB)</td>
      <td class="nu2td2">Microsoft NE2000 NDIS Driver</td>
      <td class="nu2td2">Jul 11, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Bugfix in autorun.bat</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/ep312.uha">ep312.uha</a>&nbsp;<a href="../nu2files/ep312.cab">ep312.cab</a>(7KB)</td>
      <td class="nu2td2">Surecom EP-312V Ethernet Adapter NDIS2 DOS Driver V2.72</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Dennis Ploeger</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/ibmtok.uha">ibmtok.uha</a>&nbsp;<a href="../nu2files/ibmtok.cab">ibmtok.cab</a>(12KB)</td>
      <td class="nu2td2">IBM ISA Token Ring Driver</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Pascal de Wild</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/ibmtokcb.uha">ibmtokcb.uha</a>&nbsp;<a href="../nu2files/ibmtokcb.cab">ibmtokcb.cab</a>(48KB)</td>
      <td class="nu2td2">IBM 16/4 Token ring CardBus Adapter</td>
      <td class="nu2td2">May 8, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Philippe Deplanque from IBM
        Vienna. Supports the 32 bits IBM token ring Cardbus adapter</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/ibmtokcs.uha">ibmtokcs.uha</a>&nbsp;<a href="../nu2files/ibmtokcs.cab">ibmtokcs.cab</a>(20KB)</td>
      <td class="nu2td2">IBM Auto and Turbo 16/4 Token ring PC Card and PC Card
        2</td>
      <td class="nu2td2">May 8, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Philippe Deplanque from IBM
        Vienna. Is supposed to cover the 16bits pcmcia token ring cards. It is
        tested on the 3 families: IBM auto 16/4 PC Card, IBM turbo 16/4 PC Card
        and IBM turbo 16/4 PC Card 2.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/ibmtrp.uha">ibmtrp.uha</a>&nbsp;<a href="../nu2files/ibmtrp.cab">ibmtrp.cab</a>(39KB)</td>
      <td class="nu2td2">IBM Token-Ring PCI Family Adapter (IBMTRP.DOS)</td>
      <td class="nu2td2">Mar 27, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Van den Ende Jacques</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/ibmcndis.uha">ibmcndis.uha</a>&nbsp;<a href="../nu2files/ibmcndis.cab">ibmcndis.cab</a>(24KB)</td>
      <td class="nu2td2">IBM 10/100 EtherJet CardBus Adapter (08L3147)</td>
      <td class="nu2td2">Apr 24, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Dieter de Sena. Product: Ethernet
        Adapters(PCMCIA-08L3147) <a title="http://www.pc.ibm.com/qtechinfo/MIGR-4GJS2U.html" href="http://www.pc.ibm.com/qtechinfo/MIGR-4GJS2U.html" target="_blank">More
        info!</a></td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/ibmfe.uha">ibmfe.uha</a>&nbsp;<a href="../nu2files/ibmfe.cab">ibmfe.cab</a>(12KB)</td>
      <td class="nu2td2">IBM 100/10 EtherJet PCI Adapter Driver</td>
      <td class="nu2td2">Jul 5, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Kapa.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/ibmeindi.uha">ibmeindi.uha</a>&nbsp;<a href="../nu2files/ibmeindi.cab">ibmeindi.cab</a>(8KB)</td>
      <td class="nu2td2">IBM EtherJet ISA Ethernet driver V2.24</td>
      <td class="nu2td2">Aug 2, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Joao Claudio Pizzato Sidou.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/xj10bt.uha">xj10bt.uha</a>&nbsp;<a href="../nu2files/xj10bt.cab">xj10bt.cab</a>(15KB)</td>
      <td class="nu2td2">Megahertz XJ10BT &amp; CC10BT PC Card (Small - Enabler
        v1.30)</td>
      <td class="nu2td2">Mar 27, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Wes Brewer<br>
        Megahertz drivers with the older point enabler v1.30 which is a lot
        smaller then the new version but doesn't support as many PC Card
        controllers.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/xj10bt2.uha">xj10bt2.uha</a>&nbsp;<a href="../nu2files/xj10bt2.cab">xj10bt2.cab</a>(36KB)</td>
      <td class="nu2td2">Megahertz XJ10BT &amp; CC10BT PC Card (Large - Enabler
        v2.05)</td>
      <td class="nu2td2">Mar 27, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Wes Brewer<br>
        Megahertz drivers with the new point enabler v2.05 which is huge but
        supports newer PC Card Controllers.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/oct3xnd2.uha">oct3xnd2.uha</a>&nbsp;<a href="../nu2files/oct3xnd2.cab">oct3xnd2.cab</a>(40KB)</td>
      <td class="nu2td2">Olicom 3139/314x/3250/3540 Token-Ring 16/4 Adapter</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Ralf Jungmann</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/oce4x.uha">oce4x.uha</a>&nbsp;<a href="../nu2files/oce4x.cab">oce4x.cab</a>(9KB)</td>
      <td class="nu2td2">Olicom OC-2326 Driver</td>
      <td class="nu2td2">Apr 9, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Douglas Earnshaw</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/oce5xnd2.uha">oce5xnd2.uha</a>&nbsp;<a href="../nu2files/oce5xnd2.cab">oce5xnd2.cab</a>(17KB)</td>
      <td class="nu2td2">OC-2327 Rapidfire 10/100 Ethernet Adapter</td>
      <td class="nu2td2">Sep 3, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Andrew Chittams.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/olitok16.uha">olitok16.uha</a>&nbsp;<a href="../nu2files/olitok16.cab">olitok16.cab</a>(38KB)</td>
      <td class="nu2td2">Olicom OC-3137 Token-Ring 16/4 PCI/II Adapter</td>
      <td class="nu2td2">May 24, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Chris Gepp</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/olitokr.uha">olitokr.uha</a>&nbsp;<a href="../nu2files/olitokr.cab">olitokr.cab</a>(39KB)</td>
      <td class="nu2td2">Olicom OC-3118 ISA Adapter</td>
      <td class="nu2td2">May 24, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Chris Gepp</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/mdgnd.uha">mdgnd.uha</a>&nbsp;<a href="../nu2files/mdgnd.cab">mdgnd.cab</a>(130KB)</td>
      <td class="nu2td2">Madge Token-Ring DOS NDIS MAC Driver v5.17</td>
      <td class="nu2td2">Apr 4, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Pascal de Wild (v1.0) and Keith
        Edmunds (v1.1)</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/fa31x.uha">fa31x.uha</a>&nbsp;<a href="../nu2files/fa31x.cab">fa31x.cab</a>(15KB)</td>
      <td class="nu2td2">FA31X 10/100 MacPhyter PCI Adapters DOS v1.05</td>
      <td class="nu2td2">May 21, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Ken Wygant. Updated by Eric
        Gentry.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/ngrpci.uha">ngrpci.uha</a>&nbsp;<a href="../nu2files/ngrpci.cab">ngrpci.cab</a>(16KB)</td>
      <td class="nu2td2">Netgear FA310TX Fast Ethernet PCI Adapter</td>
      <td class="nu2td2">Apr 10, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Shane Brooks. Try newer driver:
        fa31x.cab</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/fa410.uha">fa410.uha</a>&nbsp;<a href="../nu2files/fa410.cab">fa410.cab</a>(12KB)</td>
      <td class="nu2td2">Netgear FA410TX PCMCIA Mobile Adapter v3.0</td>
      <td class="nu2td2">Aug 29, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Carl Sawyer.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/fa411.uha">fa411.uha</a>&nbsp;<a href="../nu2files/fa411.cab">fa411.cab</a>(11KB)</td>
      <td class="nu2td2">Netgear FA411 PCMCIA Mobile Adapter v3.0</td>
      <td class="nu2td2">Jul 5, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Dennis Diaz.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/endsxx.uha">endsxx.uha</a>&nbsp;<a href="../nu2files/endsxx.cab">endsxx.cab</a>(10KB)</td>
      <td class="nu2td2">Crystal LAN(tm) CS8900/CS8920 Ethernet Adapter</td>
      <td class="nu2td2">Mar 26, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Jim Webster. It was tested with
        an IO address of 300 and interrupt 10.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/fastnic.uha">fastnic.uha</a>&nbsp;<a href="../nu2files/fastnic.cab">fastnic.cab</a>(8KB)</td>
      <td class="nu2td2">ADMtek PCI 10/100 Fast Ethernet Adapter Driver v1.05</td>
      <td class="nu2td2">Apr 4, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2"><a title="http://www.admtek.com/Download.htm" href="http://www.admtek.com/Download.htm" target="_blank">More
        info!</a></td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/le100.uha">le100.uha</a>&nbsp;<a href="../nu2files/le100.cab">le100.cab</a>(14KB)</td>
      <td class="nu2td2">Trust MB100 Network PC-Card (Large - Enabler v2.05)</td>
      <td class="nu2td2">Apr 23, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Marco Gubitzer</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/at2400.cab">at2400.cab</a>&nbsp;<a href="../nu2files/at2400.cab">at2400.cab</a>(7KB)</td>
      <td class="nu2td2">Allied Telesyn AT2400 PCI</td>
      <td class="nu2td2">May 10, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Ben Pauly.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/hpfend.uha">hpfend.uha</a>&nbsp;<a href="../nu2files/hpfend.cab">hpfend.cab</a>(14KB)</td>
      <td class="nu2td2">Hewlett-Packard 10/100VG NDIS 2.01 Driver</td>
      <td class="nu2td2">May 31, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Daniel Homolka.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/uk0022.uha">uk0022.uha</a>&nbsp;<a href="../nu2files/uk0022.cab">uk0022.cab</a>(9KB)</td>
      <td class="nu2td2">ETHNE$ - Unisys custom NE2000 chip for 486s</td>
      <td class="nu2td2">May 31, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Al Gilhousen. UK0022 driver works
        best for both the 486 and pentium versions of the Unisys box but the
        UK0023 version sometimes works in situations that the UK0022 does not
        (the chips are marked uk0022 or uk0023).</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/uk0023.uha">uk0023.uha</a>&nbsp;<a href="../nu2files/uk0023.cab">uk0023.cab</a>(9KB)</td>
      <td class="nu2td2">ETHNE$ - Unisys NE2000 driver for Pentiums (no emm386!)</td>
      <td class="nu2td2">May 31, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Al Gilhousen. UK0022 driver works
        best for both the 486 and pentium versions of the Unisys box but the
        UK0023 version sometimes works in situations that the UK0022 does not
        (the chips are marked uk0022 or uk0023).</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/a2500.uha">a2500.uha</a>&nbsp;<a href="../nu2files/a2500.cab">a2500.cab</a>(21KB)</td>
      <td class="nu2td2">Allied Tsyn PCI Ethernet Adapter</td>
      <td class="nu2td2">Jul 4, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Homan Tashakoor.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/rl100a.uha">rl100a.uha</a>&nbsp;<a href="../nu2files/rl100a.cab">rl100a.cab</a>(7KB)</td>
      <td class="nu2td2">Compex RL100ATX 10/100Base-TX PCI Fast Ethernet Adapter</td>
      <td class="nu2td2">Jul 5, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Mikhail Tungusov.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/rlpnpa.uha">rlpnpa.uha</a>&nbsp;<a href="../nu2files/rlpnpa.cab">rlpnpa.cab</a>(8KB)</td>
      <td class="nu2td2">Compex RL2000A PnP Ethernet Adapter NDIS driver v2.10
        (970312)</td>
      <td class="nu2td2">Sep 4, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Rudy Tuypens.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/aln325.uha">aln325.uha</a>&nbsp;<a href="../nu2files/aln325.cab">aln325.cab</a>(21KB)</td>
      <td class="nu2td2">AcerLAN 325 10/100 PCI</td>
      <td class="nu2td2">Jul 5, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Robert Cooper</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/rl2000.uha">rl2000.uha</a>&nbsp;<a href="../nu2files/rl2000.cab">rl2000.cab</a>(6KB)</td>
      <td class="nu2td2">Compex RL2000 PCI Ethernet Adapter NDIS Driver v1.10
        (960416)</td>
      <td class="nu2td2">Sep 3, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Peter Waeltken.</td>
    </tr>
    <tr>
      <td class="nu2td2" rowSpan="2"><a href="../nu2files/epxet.uha">epxet.uha</a>&nbsp;<a href="../nu2files/epxet.cab">epxet.cab</a>(8KB)</td>
      <td class="nu2td2">EigerNet Lan Adapter EPX-10BT NDIS 2.0.1 Driver, v2.10</td>
      <td class="nu2td2">Sep 4, 2002</td>
    </tr>
    <tr>
      <td class="nu2td" colSpan="2">Created by Angelo Sarto. Settings in
        epxet.ini: INT=5/PORT=0x300/MEM=0xD0000</td>
    </tr>
  </tbody>
</table>
<br>
<p>&nbsp;</p>
<!--webbot bot="Include" U-Include="footer.htm" TAG="BODY" startspan -->

<hr>
<font size="1">
 Copyright © 2001-2005 Tom Ehlert Software -- last modified 12 Nov 05</font> 

<a href="botindex.htm" style="color:white">link table for Bots</a>

<script type="text/javascript">
<!--
function IncludeOuterFrames(){
var loaded=top.location.pathname;
var start = 0;

for (var i = loaded.length-1;i >= 0; i--)
	{
	if (loaded.substring(i,i+1) == "/" || loaded.substring(i,i+1) == "\\")
		{
		start = i+1;
		break;
		}	
	}
if (loaded.substring(start,start+1) != "i") 	return;
if (loaded.substring(start,start+10) == "index.htm") 	return;
if (loaded.substring(start,start+10) == "intro.htm") 	return;
top.location.replace(loaded.substring(start+1,loaded.length));
}

IncludeOuterFrames();

//-->  
</script>



<!--webbot bot="Include" endspan i-checksum="23597" -->

</html>
